../Drivers/CMSIS/Include/core_cm0.h:623:22:__NVIC_EnableIRQ	16	static
../Drivers/CMSIS/Include/core_cm0.h:659:22:__NVIC_DisableIRQ	16	static,ignoring_inline_asm
../Drivers/CMSIS/Include/core_cm0.h:678:26:__NVIC_GetPendingIRQ	16	static
../Drivers/CMSIS/Include/core_cm0.h:697:22:__NVIC_SetPendingIRQ	16	static
../Drivers/CMSIS/Include/core_cm0.h:712:22:__NVIC_ClearPendingIRQ	16	static
../Drivers/CMSIS/Include/core_cm0.h:730:22:__NVIC_SetPriority	24	static
../Drivers/CMSIS/Include/core_cm0.h:754:26:__NVIC_GetPriority	16	static
../Drivers/CMSIS/Include/core_cm0.h:856:34:__NVIC_SystemReset	8	static,ignoring_inline_asm
../Drivers/CMSIS/Include/core_cm0.h:920:26:SysTick_Config	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:135:6:HAL_NVIC_SetPriority	24	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:151:6:HAL_NVIC_EnableIRQ	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:167:6:HAL_NVIC_DisableIRQ	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:180:6:HAL_NVIC_SystemReset	8	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:193:10:HAL_SYSTICK_Config	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:225:10:HAL_NVIC_GetPriority	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:238:6:HAL_NVIC_SetPendingIRQ	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:256:10:HAL_NVIC_GetPendingIRQ	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:272:6:HAL_NVIC_ClearPendingIRQ	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:289:6:HAL_SYSTICK_CLKSourceConfig	16	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:307:6:HAL_SYSTICK_IRQHandler	8	static
../Drivers/STM32F0xx_HAL_Driver/Src/stm32f0xx_hal_cortex.c:316:13:HAL_SYSTICK_Callback	8	static
